[20210118]

1.  Only for chip SA9227
2.  Manufacture string: "HDCVT".
3.  Product string: "DETHONRAY Honey H1".
4.  Audio interface string: "DETHONRAY Honey H1".
5.  Vendor ID : "0x262A".
6.  Product ID: "0x9227"(High Speed)¡B"0x9217"(Full Speed).
7.  Support playback 44.1kHz - 384kHz (16 bit/24 bit/32 bit).
*8.  Support DSD(Dop, Native DSD, Raw DSD).
9.  No Record.
10. Async mode.
11. GPIO4 : Previous song.
    GPIO5 : Next song.
    GPIO6 : P/P.
*12. Output type -> headphone.
*13. No AC3/DTS.

=================================================================

[20200924]

1.  Only for chip SA9227
2.  Manufacture string: "HDCVT".
3.  Product string: "DETHONRAY Honey H1".
4.  Audio interface string: "DETHONRAY Honey H1".
5.  Vendor ID : "0x262A".
6.  Product ID: "0x9227"¡]High Speed¡^¡B"0x9217"¡]Full Speed¡^.
*7.  Support playback 44.1kHz - 384kHz (16 bit/24 bit/32 bit)¡BDoP.
8.  No Record.
9.  Async mode.
10. GPIO4 : Previous song.
    GPIO5 : Next song.
    GPIO6 : P/P.
11. Change GPIO 1 Control time.

=================================================================

[20200804]

1.  Only for chip SA9227
2.  Manufacture string: "HDCVT".
3.  Product string: "DETHONRAY Honey H1".
4.  Audio interface string: "DETHONRAY Honey H1".
5.  Vendor ID : "0x262A".
6.  Product ID: "0x9227"¡]High Speed¡^¡B"0x9217"¡]Full Speed¡^.
7.  Support playback 44.1kHz - 384kHz (16 bit/24 bit/32 bit)¡BDSD.
8.  No Record.
9.  Async mode.
10. GPIO4 : Previous song.
    GPIO5 : Next song.
    GPIO6 : P/P.
11. Change GPIO 1 Control time.

=================================================================

[20200603]

1.  Only for chip SA9227
2.  Manufacture string: ¡§HDCVT¡¨.
3.  Product string: ¡§DETHONRYA Honey H1¡¨.
4.  Audio interface string: ¡§DETHONRYA Honey H1¡¨.
5.  Vendor ID : ¡§0x262A¡¨.
6.  Product ID: ¡§0x9227¡¨¡]High Speed¡^¡B¡§0x9217¡¨¡]Full Speed¡^.
7.  Support playback 44.1kHz - 384kHz (16 bit/24 bit/32 bit)¡BDSD.
8.  No Record.
9.  Async mode.
10. GPIO4 : Vol+.
    GPIO5 : Vol-.
    GPIO6 : P/P.